Navigation: Domain > Domain Settings > General Settings > Miscellaneous |

Enable FXP

Allow FTP transfer from server to server directly, you need to enable it while using Wing Gateway as a FTP reverse proxy.

FTP for Windows Explorer uses UTF-8 (Windows)

You can disable this option to improve Unicode compatibility when using Windows Explorer.

Enable FTP command 'AUTH TLS/SSL'

Allow the FTP command 'AUTH TLS/SSL', it is required for the FTPES protocol.

FTP's file timestamp uses GMT time

FTP's file listing shows the GMT timestamp by default. If not checked, the local time will be used instead.

Use customized logo

You can specify a custom logo to be displayed in Web Client (for this domain).

Enable HTTP welcome message

You can enable this option and define the welcome message, then logged in HTTP(S) sessions will see the message. Supported HTML tags: <h1>~<h6>, <strong>, <span>, <em>, <b>, <i>, <u>, <p>.

Transfer buffer size

Transfer buffer size used to transfer data (default is 65535). You can increase this value if you want the server to read/write less often from/to the local storage.

SSH (SFTP) banner

You can define your own SSH (SFTP) banner string here.

SSL Certificate

Select an SSL certificate for this domain. You can manage your SSL certificates in "Server > Settings > SSL certificate manager". An SSL certificate is used for FTPS/HTTPS.

SSH Host Key

Select an SSH host key for this domain. You can manage your SSH host keys at "Server > Settings > SSH host key manager". An SSH host key is used for the SFTP connection.

SMTP Configuration

Select an SMTP configuration for this domain. You can manage your SMTP configurations at "Server > Settings > SMTP configuration manager". An SMTP configuration is used for sending emails.

Enable MODE Z compression

FTP extension command "MODE Z" is used to compress the transfer data.

Default compression level

If FTP client does not specify the compression level, the server will use this default value.

Maximum and Minimum allowed compression level

The maximum and minimum allowed compression level can set from 1 to 9.